/******************************************************************************
  Filename:       interrupt_stubs.s51
  Revised:        $Date: 2011-07-15 18:33:23 -0700 (Fri, 15 Jul 2011) $
  Revision:       $Revision: 26810 $

  Description:    Interrupt vectors for CC253x Boot Code.


  Copyright 2010-2011 Texas Instruments Incorporated. All rights reserved.

  IMPORTANT: Your use of this Software is limited to those specific rights
  granted under the terms of a software license agreement between the user
  who downloaded the software, his/her employer (which must be your employer)
  and Texas Instruments Incorporated (the "License").  You may not use this
  Software unless you agree to abide by the terms of the License. The License
  limits your use, and you acknowledge, that the Software may not be modified,
  copied or distributed unless embedded on a Texas Instruments microcontroller
  or used solely and exclusively in conjunction with a Texas Instruments radio
  frequency transceiver, which is integrated into your product.  Other than for
  the foregoing purpose, you may not use, reproduce, copy, prepare derivative
  works of, modify, distribute, perform, display or sell this Software and/or
  its documentation for any purpose.

  YOU FURTHER ACKNOWLEDGE AND AGREE THAT THE SOFTWARE AND DOCUMENTATION ARE
  PROVIDED “AS IS” WITHOUT WARRANTY OF ANY KIND, EITHER EXPRESS OR IMPLIED,
  INCLUDING WITHOUT LIMITATION, ANY WARRANTY OF MERCHANTABILITY, TITLE,
  NON-INFRINGEMENT AND FITNESS FOR A PARTICULAR PURPOSE. IN NO EVENT SHALL
  TEXAS INSTRUMENTS OR ITS LICENSORS BE LIABLE OR OBLIGATED UNDER CONTRACT,
  NEGLIGENCE, STRICT LIABILITY, CONTRIBUTION, BREACH OF WARRANTY, OR OTHER
  LEGAL EQUITABLE THEORY ANY DIRECT OR INDIRECT DAMAGES OR EXPENSES
  INCLUDING BUT NOT LIMITED TO ANY INCIDENTAL, SPECIAL, INDIRECT, PUNITIVE
  OR CONSEQUENTIAL DAMAGES, LOST PROFITS OR LOST DATA, COST OF PROCUREMENT
  OF SUBSTITUTE GOODS, TECHNOLOGY, SERVICES, OR ANY CLAIMS BY THIRD PARTIES
  (INCLUDING BUT NOT LIMITED TO ANY DEFENSE THEREOF), OR OTHER SIMILAR COSTS.

  Should you have any questions regarding your right to use this Software,
  contact Texas Instruments Incorporated at www.TI.com.
******************************************************************************/

OFFSET   EQU    0x800

                COMMON  INTVEC(1)
                ;
                ; interrupt vectors in boot code simply jump to the user's LJMP
                ; instruction based at the known offset of 0x800 (flash page 1).
                ;
                ; the boot code does not use interrupts.

   ORG     0x0003      ; RF Tx FIFO underflow and overflow
   LJMP  $ + OFFSET
   ORG     0x000B      ; ADC end of conversion
   LJMP  $ + OFFSET
   ORG     0x0013      ; USART0 Rx complete
   LJMP  $ + OFFSET
   ORG     0x001B      ; USART1 Rx complete
   LJMP  $ + OFFSET
   ORG     0x0023      ; AES encryption/decryption complete
   LJMP  $ + OFFSET
   ORG     0x002B      ; Sleep timer compare
   LJMP  $ + OFFSET
   ORG     0x0033      ; Port 2 inputs
   LJMP  $ + OFFSET
   ORG     0x003B      ; USART0 Tx complete
   LJMP  $ + OFFSET
   ORG     0x0043      ; DMA transfer complete
   LJMP  $ + OFFSET
   ORG     0x004B      ; Timer 1 (16-bit) capture/compare/overflow
   LJMP  $ + OFFSET
   ORG     0x0053      ; Timer 2 (MAC timer)
   LJMP  $ + OFFSET
   ORG     0x005B      ; Timer 3 (8-bit) capture/compare/overflow
   LJMP  $ + OFFSET
   ORG     0x0063      ; Timer 4 (8-bit) capture/compare/overflow
   LJMP  $ + OFFSET
   ORG     0x006B      ; Port 0 inputs
   LJMP  $ + OFFSET
   ORG     0x0073      ; USART1 Tx complete
   LJMP  $ + OFFSET
   ORG     0x007B      ; Port 1 inputs
   LJMP  $ + OFFSET
   ORG     0x0083      ; RF general interrupts
   LJMP  $ + OFFSET
   ORG     0x008B      ; Watchdog overflow in timer mode
   LJMP  $ + OFFSET

   END
