;
; Texas Instruments CC2531 Low-power RF to USB Serial Port example setup file
;
; based on Windows USB CDC ACM Setup file
; Copyright (c) 2000 Microsoft Corporation
; Copyright (C) 2009 Texas Instruments Inc

[Version]
Signature="$Windows NT$"
Class=Ports
ClassGuid={4D36E978-E325-11CE-BFC1-08002BE10318}
Provider=%PROVIDER%
LayoutFile=layout.inf
DriverVer=05/01/2009,1.1.0.0

[Manufacturer]
%MFGNAME%=DeviceList, NTx86, NTia64, NTamd64

[DestinationDirs]
DefaultDestDir=12

[SourceDisksFiles]

[SourceDisksNames]

[DeviceList.NTx86]
%DESCRIPTION%=DriverInstall, USB\VID_0451&PID_16A8

[DeviceList.NTia64]
%DESCRIPTION%=DriverInstall, USB\VID_0451&PID_16A8

[DeviceList.NTamd64]
%DESCRIPTION%=DriverInstall, USB\VID_0451&PID_16A8


;------------------------------------------------------------------------------
;  32-bit section for Windows 2000/2003/XP/Vista
;------------------------------------------------------------------------------

[DriverInstall.NTx86]
include=mdmcpq.inf
CopyFiles=DriverCopyFiles
AddReg=DriverInstall.NTx86.AddReg

[DriverInstall.NTx86]
include=mdmcpq.inf
CopyFiles=DriverCopyFiles
AddReg=DriverInstall.NTx86.AddReg

[DriverCopyFiles]
usbser.sys,,,0x20

[DriverInstall.NTx86.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,usbser.sys
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"

[DriverInstall.NTx86.Services]
AddService=usbser, 0x00000002, DriverService

;------------------------------------------------------------------------------
;  64-bit section for Intel Itanium based systems
;------------------------------------------------------------------------------

[DriverInstall.NTia64]
include=mdmcpq.inf
CopyFiles=DriverCopyFiles
AddReg=DriverInstall.NTia64.AddReg

[DriverInstall.NTia64]
include=mdmcpq.inf
CopyFiles=DriverCopyFiles
AddReg=DriverInstall.NTia64.AddReg

[DriverCopyFiles]
usbser.sys,,,0x20

[DriverInstall.NTia64.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,usbser.sys
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"

[DriverInstall.NTia64.Services]
AddService=usbser, 0x00000002, DriverService

;------------------------------------------------------------------------------
;  64-bit section for AMD64 and Intel EM64T based systems
;------------------------------------------------------------------------------

[DriverInstall.NTamd64]
include=mdmcpq.inf
CopyFiles=DriverCopyFiles
AddReg=DriverInstall.NTamd64.AddReg

[DriverInstall.NTamd64]
include=mdmcpq.inf
CopyFiles=DriverCopyFiles
AddReg=DriverInstall.NTamd64.AddReg

[DriverCopyFiles]
usbser.sys,,,0x20

[DriverInstall.NTamd64.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,usbser.sys
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"

[DriverInstall.NTamd64.Services]
AddService=usbser, 0x00000002, DriverService

;------------------------------------------------------------------------------
;
;------------------------------------------------------------------------------

[DriverService]
DisplayName=%SERVICE%
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\usbser.sys			;;%12% == "%WINDIR%\system32\"

;------------------------------------------------------------------------------
;  String Definitions
;------------------------------------------------------------------------------

[Strings]
PROVIDER="Texas Instruments"
MFGNAME="Texas Instruments"
DESCRIPTION="TI CC2531 Low-Power RF to USB CDC Serial Port"
SERVICE="TI CC2531 Low-Power RF to USB CDC Serial Port"
